CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Mon Mar 14 11:53:00 2016
Release      : TOPSPIN Version 3.2-pl5
Installed in : /opt/topspin3.2
Host         : avIII600
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : vasenkov (Segey Vasenkov)
Description  : Avance-AV 600
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 600.03 MHz
Order Number : 10051324
Configured in: /opt/topspin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.251
- Tctrl : 1
- Fctrls: 3
- Gctrl1: with digital preemphasis
- Gctrl2: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU: AQS DRU-E Z102520/02689 ECL 06.02
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  5.1 REC-1  AQS RXAD600 Z102117/1299 ECL 05.01
     3   0x34 0xc0   0x1        X  2.3 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AD  S  2.8 SGU-1  AQS SGU/2 600 Z103081/02934 ECL 02.08 FPGA-Vs=AF
     5   0x25 0x19   0x8    AD  S  2.8 SGU-2  AQS SGU/2 600 Z103081/02935 ECL 02.08 FPGA-Vs=AF
     6   0x26 0x19   0x8    AD  S  2.8 SGU-3  AQS SGU/2 600 Z103081/02936 ECL 02.08 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345509_0016 W1345509/0016 ECL 10:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAH500 E 500-600MHZ INR: W1345509/0016 ECL 10
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1582 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5665 ECL 50
BLA_W1345094_0089 W1345094/0089 ECL 11:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLA2X500 E 6-365MHZ INR: W1345094/0089 ECL 11
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1371 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6091 ECL 50
LTRX Z109890/00244 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00244 ECL 02.01

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGAU_W1522066_0077
- TCP/IP address   = 149.236.99.250
- Firmware version = BGMUI1_20140415b (unknown format, update may be necessary)
- Web version      = 2.1
- Current limits   = 60.0/X, 60.0/Y, 60.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130627
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00244 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00734 ECL 03.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00836 ECL 01.03

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

MAS2 control unit: connected to 149.236.99.251:/dev/tty04
- Boot Software        : 20100908
- Application Software : 20090331
- Insert Time          : 10 s
- Eject Time           : 10 s
- Spin Lock Tolerance  : 5 Hz

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.1%/0.1deg, reflection meter)
                 PN=Z103205, SN=00086 from 20111205
    Module  2 : 2H
                 PN=Z003473, SN=00890 from 20111124
    Module  3 : XBB19F 2HS
                 PN=Z003506, SN=01048 from 20111109
    Module  4 : 13C
                 PN=Z003524, SN=00696 from 20111126
    Module  5 : 19F
                 PN=Z003495, SN=00009 from 20060607


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0089 at TCP/IP 149.236.99.252)
SGU1 AUX  output -> input 1 of transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00244 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 1 of transmitter 1 (BLAH500 E 500-600MHZ INR W1345509/0016 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0089 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> open

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAH500 E 500-600MHZ INR W1345509/0016 at TCP/IP 149.236.99.253) amplifier 1H-500W uses blanking 2
transmitter 1 (BLAH500 E 500-600MHZ INR W1345509/0016 at TCP/IP 149.236.99.253) amplifier 1H-50W uses blanking 2
transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0089 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 1
transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0089 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 3
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00244 at TCP/IP 149.236.99.20) amplifier 2H-5W uses blanking 7

