CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Thu Jun 16 13:12:28 2016
Release      : TOPSPIN Version 3.2-pl5
Installed in : /opt/topspin3.2
Host         : av600.mbi.ufl.edu
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Pentium(R) 4 CPU 3.00GHz (1 core at 2800 MHz)
User         : nmrsu (NMR Administrator)
Description  : Avance-AV 600
Location     : McKnight Brain Institute
System       : Avance-AV NMR spectrometer
1H-frequency : 600.23 MHz
Order Number : 1
Configured in: /opt/topspin3.2/conf/instr/spect

#--------------------
#  FCU configuration:
#--------------------
board # 1 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 2 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 3 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)
board # 4 :
	MEMORY 0x1ff000	(=511 k Words)
	PAL-Version 0x104 = new version (EC level 07 or more)

DRU: AQS DRU-E Z102520/00249 ECL 03.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419

Gcu: GCU3_SlowIF

AQS: connected to spect:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x2    AW  R  1.1 REC-1  AQS RXAD600 Z102117/150 ECL 1.1
     3   0x34 0xc0   0x1        X  0.4 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x18   0x4    BG  S  4.0 SGU-1  AQS SGU600 Z003831/02334 ECL 4.0
     5   0x25 0x18   0x4    BG  S  4.1 SGU-2  AQS SGU600 Z003831/02475 ECL 4.1
     6   0x26 0x18   0x4    BG  S  4.0 SGU-3  AQS SGU600 Z003831/02359 ECL 4.0
     7   0x27 0x18   0x4    BG  S  4.0 SGU-4  AQS SGU600 Z003831/02353 ECL 4.0
     8   0x3c  0x4     0        Y  1.0 ROUT-1 Avance Router 3/5
    21   0x21  0xa     0        P  2.0 PSD-1  Power Supply Distribution Board
    23   0x20 0xc6     0        B  1.1 AQS/2  AQS/2 chassis
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 Avance-Router

Amplifier Control Board:  connected to spect:/dev/tty20


Amplifiers (ACB configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        X      300    N  (V=ff) BLAXH2H 300/100/150 W1345080/21/20050420
   2      1         2       1H      100    N  (-""-) BLAXH2H 300/100/150 W1345080/21/20050420
   3      2         1        X      300    N  (V=ff) BLAX 300 W1345069/80/20050420
   6      3         1       2H      150    N         BLAXH2H 300/100/150 W1345080/21/20000000



- Type: BSMS/1
- absolute lockshift frequency =  12138960 Hz
- GAB type = GAB
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)

Bruker Automatic Changer: device connected to spect:/dev/tty08
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 0 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - SampleJet: at TCP/IP address 149.236.99.55


Lock: device connected to spect:/dev/tty03

Eurotherm VTU: device connected to spect:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to spect:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00743 from 20130531
    Module  2 : XBB19F 2HS
                 PN=Z003506, SN=68 from 20010620
    Module  3 : 2H
                 PN=Z003473, SN=00490 from 20061206
    Module  4 : 13C
                 PN=Z003524, SN=20 from 20010614
    Module  5 : 15N
                 PN=Z003530, SN=20 from 20010615


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



