CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Tue Jul 23 17:28:36 2019
Release      : TOPSPIN Version 3.2-pl5
Installed in : C:/Bruker/TopSpin3.2
Host         : CZC345D12M
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 3591 MHz with Hyperthreading)
User         : nmr
Description  : AVIIIHD850
Location     : Xiamen University, China
System       : Avance III NMR spectrometer
1H-frequency : 850.29 MHz
Order Number : 10091421
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.251
- Tctrl : 1
- Fctrls: 5
- Gctrl1: with digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : 1

DRU: AQS DRU-E Z102520/03704 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.2 REC-1  AQS RXAD/2 1000 Z130589/75 ECL 00.02
     3   0x34 0xda   0x1        X  0.2 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00146 ECL 01.03 FPGA-Vs=20130829
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00217 ECL 01.03 FPGA-Vs=20131031
     6   0x28 0x33     0        S  1.3 SGU-3  AQS SGU/3 1200 (2CH) Z117130/00406 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  1.1 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0299 W1345097/0299 ECL 20:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0299 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/2029 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7777 ECL 50
BLA_W1345093_0645 W1345093/0645 ECL 12:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0645 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/2409 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/7452 ECL 50
LTRX Z109894/00025 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 850: Z109894/00025 ECL 01.01

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGA_W1213762_0158
- TCP/IP address   = 149.236.99.254
- Firmware version = 20080206
- Web version      = 1.1
- Current limits   = -10.0/X, -10.0/Y, -10.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130627
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 850: Z109894/00025 ECL 01.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03638 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02038 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.251:/dev/tty04

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.251:/dev/tty01

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.7%/-0.0deg, reflection meter)
                 PN=Z105203, SN=00044 from 20130502
    Module  2 : 2H
                 PN=Z104078, SN=00031 from 20130514
    Module  3 : XBB31P 2HS
                 PN=Z104077, SN=00035 from 20130425
    Module  4 : 15N
                 PN=Z107394, SN=00024 from 20130514
    Module  5 : 13C
                 PN=Z107393, SN=00024 from 20130603


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU
- F5: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0645 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0645 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253)
SGU4 NORM output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253)
SGU4 AUX  output -> open
SGU5 NORM output -> input 3 of transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0645 at TCP/IP 149.236.99.252)
SGU5 AUX  output -> open

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253) amplifier 1H-100W uses blanking 2
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253) amplifier X-500W uses blanking 1
transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0299 at TCP/IP 149.236.99.253) amplifier 2H-250W uses blanking 7
transmitter 2 (BLAX500 E 6-365MHZ INR W1345093/0645 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 3
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 850 Z109894/00025 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

