CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.6.2/conf/instr/spect/uxnmr.info
Date         : Thu Feb 06 15:44:20 2020
Release      : TopSpin 3.6.2
Installed in : C:/Bruker/TopSpin3.6.2
Host         : AV600B
OS           : Windows 7 (Vs 6.2)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v2 @ 3.70GHz (8 cores at 3691 MHz with Hyperthreading)
User         : nmrsu
System       : Avance III HD 600 NMR spectrometer
1H-frequency : 600.04 MHz
Description  : CABINET 600 HD X TB
Location     : Universita degli Studi di Firenze Sesto Fiorentino
Bruker Order : 10181407
Configured in: AV600B:C:/Bruker/TopSpin3.6.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/04553 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.3 REC-1  AQS RXAD/2 600 Z130588/1889 ECL 00.03
     3   0x34 0xd6   0x1        X  4.2 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  2.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/02262 ECL 02.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  2.2 SGU-2  AQS SGU/3 600 (2CH) Z117129/02263 ECL 02.02 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345083_1042 W1345083/1042 ECL 21:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH300/100 E 200-600MHZ INR: W1345083/1042 ECL 21
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/5020 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010544 ECL 50
BLA_W1345092_0752 W1345092/0752 ECL 11:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ INR: W1345092/0752 ECL 11
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/3063 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010577 ECL 50
LTRX Z109890/00768 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00768 ECL 03.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20170712
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00768 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02586 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/02918 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 1 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: SampleJet
- TCP/IP address   = 149.236.99.55

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.9%/0.3deg, reflection meter)
                PN=Z103205, SN=00596 from 20150112
    Module  2 : 2H
                PN=Z003473, SN=01344 from 20140806
    Module  3 : XBB19F 2HS
                PN=Z003506, SN=01614 from 20141223
    Module  4 : XBB19F 2HS
                PN=Z003506, SN=01619 from 20141223



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH300/100 E 200-600MHZ INR W1345083/1042 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0752 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH300/100 E 200-600MHZ INR W1345083/1042 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ INR W1345092/0752 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 1 of transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00768 at TCP/IP 149.236.99.20)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH300/100 E 200-600MHZ INR W1345083/1042 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1

transmitter 2 = BLAX300 E 6-365MHZ INR W1345092/0752 at TCP/IP 149.236.99.252:
- amplifier X-300W uses blanking 4

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00768 at TCP/IP 149.236.99.20:
- amplifier 2H-5W uses blanking 7


