CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.5/conf/instr/spect/uxnmr.info
Date         : Wed Jul 20 14:00:51 2022
Release      : TopSpin 3.6.5
Installed in : /opt/topspin3.6.5
Host         : av600wb
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 2700 MHz with Hyperthreading)
User         : nmr (NMR User)
System       : Avance III HD 600 NMR spectrometer
1H-frequency : 599.48 MHz
Description  : CABINET 600 HD X WB
Bruker Order : 10214911
Configured in: av600wb:/opt/topspin3.6.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.91
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/05124 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x43   0x5    CD  R  0.4 REC-1  AQS RXAD/2 600 Z130588/2570 ECL 00.04
     3   0x34 0xd6   0x1        X  4.2 REF-1  REF/3-600 Reference Board for AQS/3 Receiver
     4   0x24 0x32     0        S  3.2 SGU-1  AQS SGU/3 600 (2CH) Z117129/02977 ECL 03.02 FPGA-Vs=20131031
     5   0x26 0x32     0        S  3.5 SGU-2  AQS SGU/3 600 (2CH) Z117129/03977 ECL 03.05 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0655 W1345093/0655 ECL 12:
- TCP/IP address = 149.236.99.94
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0655 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/002433 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/007323 ECL 60
BLA_W1345098_0231 W1345098/0231 ECL 21:
- TCP/IP address = 149.236.99.90
- Firmware VS    = 20120627
- Amplifier      = BLAXH500/100 E 200-600MHZ INR: W1345098/0231 ECL 21
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/005502 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011448 ECL 60
- QNP-Accessory  : 1 X-input and 1 H-input
LTRX Z109890/00876 ECL 03.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00876 ECL 03.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210212
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00876 ECL 03.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00611 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03562 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.91:/dev/tty04
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 1 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.91:/dev/tty01
- (used by TopSpin)

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159072/275
- TCP/IP address   = 149.236.99.93

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 101.3%/-0.4deg, reflection meter)
                PN=Z103205, SN=00712 from 20160301
    Module  2 : 2H
                PN=Z003473, SN=01489 from 20160217
    Module  3 : XBB19F 2HP
                PN=Z105186, SN=00329 from 20180820
    Module  4 : 13C/79Br
                PN=Z003524, SN=01387 from 20201002
    Module  5 : 15N
                PN=Z003530, SN=01250 from 20201005



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH500/100 E 200-600MHZ INR W1345098/0231 at TCP/IP 149.236.99.90)
SGU1 AUX  output -> input 1 of transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00876 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH500/100 E 200-600MHZ INR W1345098/0231 at TCP/IP 149.236.99.90)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0655 at TCP/IP 149.236.99.94)
SGU3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAX500 E 6-365MHZ INR W1345093/0655 at TCP/IP 149.236.99.94:
- amplifier X-500W uses blanking 3

transmitter 2 = BLAXH500/100 E 200-600MHZ INR W1345098/0231 at TCP/IP 149.236.99.90:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00876 at TCP/IP 149.236.99.20:
- amplifier 2H-5W uses blanking 7


Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
transmitter 2 = BLAXH500/100 E 200-600MHZ INR W1345098/0231 at TCP/IP 149.236.99.90:
- amplifier X-500W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
- amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H


