CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.2/conf/instr/spect/uxnmr.info
Date         : Mon Dec 16 15:52:52 2019
Release      : TopSpin 3.6.2
Installed in : /opt/topspin3.6.2
Host         : avance800
OS           : CentOS release 5.10 (Final)
CPU          : Intel(R) Xeon(R) CPU E5-1620 0 @ 3.60GHz (8 cores at 1200 MHz with Hyperthreading)
User         : pedrol (Pedro Lamosa)
System       : Avance III 800 NMR spectrometer
1H-frequency : 800.33 MHz
Description  : Avance III 800
Bruker Order : SHJ201619
Configured in: avance800:/opt/topspin3.6.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/00527 ECL 03.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x52   0x3    AW  R  3.0 REC-1  AQS RXAD1000 Z102118/108 ECL 03.00
     3   0x34 0xc1   0x1        X  1.0 REF-1  REF-1000 Reference Board for AQS Receiver
     4   0x24 0x29   0x8    AE  S  2.0 SGU-1  AQS SGU/2 1000 Z103082/00185 ECL 02.00 FPGA-Vs=AF
     5   0x25 0x29   0x8    AE  S  2.0 SGU-2  AQS SGU/2 1000 Z103082/00189 ECL 02.00 FPGA-Vs=AF
     6   0x26 0x29   0x8    AE  S  2.0 SGU-3  AQS SGU/2 1000 Z103082/00171 ECL 02.00 FPGA-Vs=AF
     7   0x27 0x29   0x8    AE  S  2.0 SGU-4  AQS SGU/2 1000 Z103082/00162 ECL 02.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.2 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345097_0022 W1345097/0022 ECL 0:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ: W1345097/0022 ECL 0
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0106 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0287 ECL 1
BLA_W1345093_0027 W1345093/0027 ECL 0:
- TCP/IP address = 149.236.99.249
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ: W1345093/0027 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0153 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0109 ECL 1

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20180919
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/04865 ECL 05.02
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/04471 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty05
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Bruker Magnet Pump Control BMPC: device connected to 149.236.99.254:/dev/tty01

MAS2 control unit: connected to 149.236.99.254:/dev/tty04
MAS2: device not yet configured
MAS1: device could not be configured

Cryo Cooling Control Unit: CU5 - COOLING UNIT/5 Z159072/162
- TCP/IP address   = 149.236.99.247

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AO
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003465, SN=00094 from 20060329
    Module  2 : 13C/79Br
                PN=Z003527, SN=00396 from 20191001
    Module  3 : 15N
                PN=Z003533, SN=00403 from 20190912
    Module  4 : 2H
                PN=Z003476, SN=00095 from 20060719
    Module  5 : HPHP 19F/1H
                PN=Z003876, SN=00014 from 20060815
    Module  6 : HPHP XBB31P
                PN=Z003877, SN=00041 from 20060905
    Module  7 : HPHP XBB31P
                PN=Z003877, SN=00040 from 20060905
    Module  8 : QNP Function Module



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0022 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> open
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0022 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ W1345093/0027 at TCP/IP 149.236.99.249)
SGU3 AUX  output -> open
SGU4 NORM output -> input 4 of transmitter 1 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0022 at TCP/IP 149.236.99.253)
SGU4 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ W1345093/0027 at TCP/IP 149.236.99.249)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H500/100/250 E 700-900MHZ W1345097/0022 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W needs no blanking

transmitter 2 = BLAX500 E 6-365MHZ W1345093/0027 at TCP/IP 149.236.99.249:
- amplifier X-500W uses blanking 3


