                        INSTRUMENT CONTROL PARAMETERS:    QQQ
                        -------------------------------------

   D:\Data\JS\SKKU_PI_F_SCFA\231126_CC_R_D_B1\231127_SR2_B1_SIM.M
      Sun Nov 26 21:05:17 2023

Control Information
------- -----------

Sample Inlet             : GC
Injection Source         : GC ALS
Injection Location:  Front
Mass Spectrometer        : Enabled


 No Sample Prep method has been assigned to this method.


GC
GC Summary
Run Time                                     20 min
Post Run Time                                0 min

Oven
Temperature
Setpoint                                     On
(Initial)                                    40 °C
Hold Time                                    2 min
Post Run                                     240 °C
Program
#1 Rate                                      40 °C/min
#1 Value                                     95 °C
#1 Hold Time                                 1 min
#2 Rate                                      5 °C/min
#2 Value                                     140 °C
#2 Hold Time                                 1 min
#3 Rate                                      40 °C/min
#3 Value                                     240 °C
#3 Hold Time                                 3.125 min


Equilibration Time                           0.5 min
Max Temperature                              240 °C
Maximum Temperature Override                 Disabled
Slow Fan                                     Disabled

ALS
Front Injector
Syringe Size                                 10 μL
Injection Volume                             1 μL
Solvent A Washes (PreInj)                    3
Solvent A Washes (PostInj)                   3
Solvent A Volume                             8 μL
Solvent B Washes (PreInj)                    3
Solvent B Washes (PostInj)                   3
Solvent B Volume                             8 μL
Sample Washes                                0
Sample Wash Volume                           8 μL
Sample Pumps                                 0
Dwell Time (PreInj)                          0 min
Dwell Time (PostInj)                         0 min
Solvent Wash Draw Speed                      300 μL/min
Solvent Wash Dispense Speed                  3000 μL/min
Sample Wash Draw Speed                       300 μL/min
Sample Wash Dispense Speed                   3000 μL/min
Injection Dispense Speed                     6000 μL/min
Viscosity Delay                              0 sec
Sample Depth                                 Disabled
Injection Type                               Standard
L1 Airgap                                    0 μL
Solvent Wash Mode                            A-A6,B-B4

Sample Overlap
Mode                                         Sample overlap is not enabled

ALS Errors                                   Pause for user interaction

Front SS Inlet He
Mode                                         Split
Heater                                       On    280 °C
Pressure                                     On    48.745 kPa
Total Flow                                   On    6 mL/min
Septum Purge Flow                            On    3 mL/min
Gas Saver                                    On    20 mL/min after 2 min
Split Ratio                                  2 :1
Split Flow                                   2 mL/min
Liner                                        Agilent 5190-2295: 870 μL (Universal, low pressure drop, ultra i)

Thermal Aux 2 (MSD Transfer Line)
Temperature
Setpoint                                     On
(Initial)                                    280 °C


Column
Column #1
Flow
Setpoint                                     On
(Initial)                                    1 mL/min
Post Run                                     1 mL/min

Column Information                           J&W 122-3232
Description                                  DB-FFAP
Temperature Range                            0 °C—245 °C (250 °C)
Dimensions                                   30 m x 250 μm x 0.25 μm (Uncalibrated)
Column lock                                  Unlocked
In                                           Front SS Inlet He
Out                                          MSD 
(Initial)                                    40 °C
Pressure                                     48.745 kPa
Flow                                         1 mL/min
Average Velocity                             36.262 cm/sec
Holdup Time                                  1.3789 min
Control Mode                                 Constant Flow

Column Outlet Pressure                       0 kPa

Collision Cell EPC
Quench Gas He                                On    2.25 mL/min
Collision Gas N2                             On    1.5 mL/min

Signals
Signal #1:  Test Plot
Description                                  Test Plot
Save                                         Off
Data Rate                                    50 Hz
Dual Injection Assignment                    Front Sample

Signal #2: 
Description                                  None

Signal #3: 
Description                                  None

Signal #4: 
Description                                  None






                        END OF INSTRUMENT CONTROL PARAMETERS
                        ------------------------------------
