CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.6.4/conf/instr/spect/uxnmr.info
Date         : Fri Jul 28 09:23:41 2023
Release      : TopSpin 3.6.4
Installed in : C:/Bruker/TopSpin3.6.4
Host         : AVANCE600
OS           : Windows 10 Enterprise release 2009 (Vs 6.3)
CPU          : Intel(R) Core(TM) i5-2500 CPU @ 3.30GHz (4 cores at 3293 MHz)
User         : admin
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.17 MHz
Description  : Avance III 600
Location     : Campinas, Sao Paulo, Brasil
Bruker Order : 10029886
Configured in: AVANCE600:C:/Bruker/TopSpin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01124 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  5.1 REC-1  AQS RXAD600 Z102117/1165 ECL 05.01
     3   0x34 0xc0   0x1        X  2.3 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.7 SGU-1  AQS SGU/2 600 Z103081/02606 ECL 02.07 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.7 SGU-2  AQS SGU/2 600 Z103081/02607 ECL 02.07 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.7 SGU-3  AQS SGU/2 600 Z103081/02608 ECL 02.07 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345096_0756 W1345096/0756 ECL 2:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0756 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1225 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5785 ECL 50
- QNP-Accessory  : 1 X-input and 1 H-input
BLA_W1345092_0230 W1345092/0230 ECL 1:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ: W1345092/0230 ECL 1
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0676 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V H-USB: W1522050/0397 ECL 03
LTRX Z109890/00186 ECL 02.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00186 ECL 02.00

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20220429
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00186 ECL 02.00
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/00480 ECL 02.03
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/04077 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: BACS2_H15200_0141
- TCP/IP address   = 149.236.99.177
- Protocol types   = SOAP

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                PN=Z003462, SN=00093 from 20050804
    Module  2 : XBB19F 2HS
                PN=Z003506, SN=00975 from 20110511
    Module  3 : XBB19F 2HS
                PN=Z003506, SN=00974 from 20110510
    Module  4 : 2H
                PN=Z003473, SN=00796 from 20110524



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ W1345096/0756 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX300 E 6-365MHZ W1345092/0230 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ W1345096/0756 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX300 E 6-365MHZ W1345092/0230 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 4 of transmitter 1 (BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ W1345096/0756 at TCP/IP 149.236.99.253)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ W1345096/0756 at TCP/IP 149.236.99.253:
- amplifier 1H-100W uses blanking 2
- amplifier X-300W uses blanking 1
- amplifier 2H-150W needs no blanking

transmitter 2 = BLAX300 E 6-365MHZ W1345092/0230 at TCP/IP 149.236.99.252:
- amplifier X-300W uses blanking 3

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/00186 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
transmitter 1 = BLAXH2H300/100/150 E 200-600MHZ BLAX300 E 6-365MHZ W1345096/0756 at TCP/IP 149.236.99.253:
- amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
- amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
- amplifier 2H-150W can be routed to switchbox output 5 (unknown)


